[bookmark: Record_of_BIENNIAL_FLIGHT_REVIEW_(BFR)][bookmark: Demonstration_of_Continued_Competency_fo][image: ]Part 61 demonstration of continued competency for CPL 
(helicopter) — record of biennial flight review (BFR)

[bookmark: The_candidate_is_to_be_assessed_competen]The candidate is to be assessed competent in all aspects of the CPL; this may require more than one flight. Upon completion, the instructor that conducted the BFR is to make an appropriate entry in the candidate’s logbook.

	First Names
	[bookmark: Text1]     
	Total Flight Time
	     

	Surname
	     
	Expiry date of last BFR
	     

	CAA Participant number
	     
	Flight Time since last BFR
	     

	Identity verified?
	     
	Lifetime licence sighted?
	     
	Candidate’s signature
	

	Consider:
	Holds a type rating for the aircraft?
	     
	Holds a current medical?
	     
	Medical Type
	     



	Mark each item
X = not yet competent 
Instructor’s initials = competent
	Flight time
	Flight time
	Flight time
	Flight time
	Flight time

	Date (dd/mm/yyyy)
	[bookmark: Text4]     
	     
	     
	     
	     

	Personal preparation: I’m Safe, current documents
	     
	     
	     
	     
	     

	Legislation: Privileges, currency, medical, AIP, VNC
	     
	     
	     
	     
	     

	Aircraft documents
	
	
	
	
	

	Knowledge of Certificate of Airworthiness
	     
	     
	     
	     
	     

	Knowledge of Technical log
	     
	     
	     
	     
	     

	Knowledge of Flight manual, CAA forms 2173 & 2129
	     
	     
	     
	     
	     

	Airworthiness Directives
	     
	     
	     
	     
	     

	Weather and NZAIP supplements
	
	
	
	
	

	GRAFOR, TAF, METAR, NOTAMS, Go/No go
	     
	     
	     
	     
	     

	Helicopter performance
	
	
	
	
	

	Power limit, ht/velocity, seasonal effects on performance
	     
	     
	     
	     
	     

	Fuel management: required, quantity, consumption
	     
	     
	     
	     
	     

	Loading: MAUW, C of G position, load distribution
	     
	     
	     
	     
	     

	Pre-flight inspection: interior, exterior, load security
	     
	     
	     
	     
	     

	Passenger briefing: passenger supervision & briefing
	     
	     
	     
	     
	     

	Engine start and rotor engagement: checks, fire drills
	     
	     
	     
	     
	     

	Engine checks, run up and operation: clutch overrun
	     
	     
	     
	     
	     

	Pre lift-off procedures: checks, QNH, time, lookout
	     
	     
	     
	     
	     

	ATS procedures: ATIS, clearances, phraseology
	     
	     
	     
	     
	     

	Lift-off to hover: HIGE, C of G, control & power checks
	     
	     
	     
	     
	     

	Hover maneuvering: speed, height, track, pivot turns
	     
	     
	     
	     
	     

	Takeoff
	
	
	
	
	

	Normal
	     
	     
	     
	     
	     

	Crosswind
	     
	     
	     
	     
	     

	Limited power (cushion creep)
	     
	     
	     
	     
	     

	Limited power (running)
	     
	     
	     
	     
	     

	Towering
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	Climbing: ± 10 knots, ± 5 degrees, trim, T’s & P’s, lookout
	     
	     
	     
	     
	     

	Straight and level: ± 50’, ± 5 degrees, trim
	     
	     
	     
	     
	     

	Medium turns: ± 50’, coordinated, reference point
	     
	     
	     
	     
	     

	Steep turns: ± 50’, coordinated, power, reference point
	     
	     
	     
	     
	     

	Magnetic compass headings: ± 10˚, turning ± 15˚
	     
	     
	     
	     
	     

	Straight-in autorotation: ± 10 knots, RPM, recovery
	     
	     
	     
	     
	     

	180-degree autorotation: flight path, RPM, recovery
	     
	     
	     
	     
	     

	Quick stops: RPM, height, heading ± 10 degrees
	     
	     
	     
	     
	     

	Low flying: lookout, height ± 25’, ± 10 knots
	     
	     
	     
	     
	     

	Slope operations: area, control, ± 10 degrees, hazards
	     
	     
	     
	     
	     

	Confined area operations: recon, decision & aim point
	     
	     
	     
	     
	     

	Descent: ± 10 knots, ± 5 degrees, trim
	     
	     
	     
	     
	     

	Joining the circuit: checks, procedure, sit awareness
	     
	     
	     
	     
	     

	Approach and landing
	
	
	
	
	

	Normal
	     
	     
	     
	     
	     

	Limited power (running)
	     
	     
	     
	     
	     

	Zero speed
	     
	     
	     
	     
	     

	Go-round: decision, sequence, track, transition
	     
	     
	     
	     
	     

	Steep approach: aim & decision pt, conditions, angle <15
	     
	     
	     
	     
	     

	Engine failure in hover: hdg ± 30 degrees, touchdown
	     
	     
	     
	     
	     

	Shut down: checks, pax supervision, documentation
	     
	     
	     
	     
	     

	Emergencies and hazards: as applicable to type
	     
	     
	     
	     
	     

	TEM (refer web site under Pilots/Threat & Error Policy)
	     
	     
	     
	     
	     

	Radiotelephony tuning and procedures: phraseology
	     
	     
	     
	     
	     

	Lookout (critical task): situational awareness, VMC
	     
	     
	     
	     
	     

	Flight orientation: airspace boundaries, reporting pts
	     
	     
	     
	     
	     

	Pilot judgement: performance, clearances, emergencies
	     
	     
	     
	     
	     



	[bookmark: Text3]This is to certify that       has successfully completed a BFR and demonstrated competence to exercise the privileges of a CPL (Helicopter).
I confirm that I have reviewed with the candidate the relevant safety initiatives as published on the CAANZ website applicable since their last BFR.

	Instructor Name
	[bookmark: Text2]     
	Category
	     

	Instructor CAA Participant number
	     
	Helicopter Type
	
	Registration
	     

	Signature
	
	Date
	     

	Logbook endorsed?
	     
	Next BFR due
	     



The instructor certifying competency is to distribute copies of this form as follows:
1. Candidate
2. The instructor conducting the BFR
3. Scan and email a copy to pft.admin@caa.govt.nz

Note: If Air Law KDRs are required, attach a signed copy by an A or B Cat instructor with evidence of knowledge improvement.
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